Convenience Net Lower Retainer Replacement. Opel Sintra 1999

For 1990-2009 cars

### Removal Procedure

1. Open the liftgate.
2. Remove the convenience net from the retainers.
3. Remove the nut from the floor convenience net retainer stud.
4. Remove the convenience net floor retainer from the floor.

### Installation Procedure

1. Install the convenience net floor retainer to the stud in the floor.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the nut to the floor convenience net retainer stud.

Tighten
Tighten the nut to 10 N·m (89 lb in).

3. Install the convenience net to the retainers.
4. Close the liftgate.