Transmission Mount Bracket Replacement. Opel Sintra 1999

For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the left front tire and wheel.

• | For vehicles with steel wheels, refer to Tire and Wheel Removal and Installation in Tires and Wheels.

• | For Chevrolet and Oldsmobile vehicles with aluminum wheels, refer to Tire and Wheel Removal and Installation in Tires and Wheels.

• | For Pontiac and Export vehicles with aluminum wheels, refer to Tire and Wheel Removal and Installation in Tires and Wheels.

3. Remove the left engine splash shield. Refer to Engine Splash Shield Replacement in Body Front End.
4. Use a utility stand with a block of wood in order to support the transaxle.
5. Remove the transaxle mount upper nuts.
6. Remove the transaxle mount bracket bolts.
7. Remove the transaxle mount bracket.

### Installation Procedure

1. Position the transaxle mount bracket.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the transaxle mount bracket bolts.

Tighten
Start with the forward lower bolt and work clockwise to tighten the transaxle mount bracket bolts to 95 N·m (70 lb ft).

3. Remove the utility stand.
4. Install the transaxle mount upper nuts.

Tighten
Tighten the transaxle mount upper nuts to 47 N·m (35 lb ft).

5. Install the left engine splash shield. Refer to Engine Splash Shield Replacement in Body Front End.
6. Install the left front tire and wheel.

• | For vehicles with steel wheels, refer to Tire and Wheel Removal and Installation in Tires and Wheels.

• | For Chevrolet and Oldsmobile vehicles with aluminum wheels, refer to Tire and Wheel Removal and Installation in Tires and Wheels.

• | For Pontiac and Export vehicles with aluminum wheels, refer to Tire and Wheel Removal and Installation in Tires and Wheels.

7. Lower the vehicle.