Exhaust Tail Pipe Hanger Replacement. Opel Sintra 1999

For 1990-2009 cars

## Exhaust Tail Pipe Hanger Replacement Domestic

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the tail pipe hanger insulator from the tail pipe.
3. Remove the tail pipe hanger bolts.
4. Remove the tail pipe hanger.

### Installation Procedure

1. Install the tail pipe hanger.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the tail pipe hanger bolts.

Tighten
Tighten the tail pipe hanger bolts to 50 N·m (37 lb ft).

3. Install the tail pipe hanger insulator to the tail pipe.
4. Lower the vehicle.

## Exhaust Tail Pipe Hanger Replacement Export

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the tail pipe hanger insulator from the tail pipe.
3. Remove the tail pipe hanger bolts.
4. Remove the tail pipe hanger.

### Installation Procedure

1. Install the tail pipe hanger.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the tail pipe hanger bolts.

Tighten
Tighten the tail pipe hanger bolts to 50 N·m (37 lb ft).

3. Install the tail pipe hanger insulator to the tail pipe.
4. Lower the vehicle.