Power Window Inoperative - Right Side Front. Opel Sintra 1999

For 1990-2009 cars

## Power Window Inoperative - Right Side Front from RF window switch only

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the entire power windows system check performed? | -- | Go to Step 2 | Go to Power Windows System Check

2

1. Place the ignition switch into the RUN position.
2. Using a test light, backprobe the RF window switch connector from terminal F to ground.

Does the test light illuminate?

--

Go to Step 3

Go to Step 4

3 | Replace the RF window switch. Refer to Door Trim Plate Replacement . Is the repair complete? | -- | Go to Step 5 | --
4 | Repair the open in CKT 141, between the RF window switch and S307. Is the repair complete? | -- | Go to Step 5 | --

5

1. Turn the ignition switch to the OFF position.
2. Reconnect all connectors/components removed.

Have all the repairs been made?

--

Go to Power Windows System Check

--

## Power Window Inoperative - Right Side Front from LF window switch only

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the entire power windows system check performed? | -- | Go to Step 2 | Go to Power Windows System Check

2

1. Disconnect the LF window switch.
2. Disconnect the RF window switch.
3. Check for a short to ground in CKT 166 and 167.

Is a short to ground present?

--

Go to Step 3

Go to Step 4

3 | Repair the short to ground. Is the repair complete? | -- | Go to Step 5 | --
4 | Replace the LF window switch. Refer to Door Trim Plate Replacement . Is the repair complete? | -- | Go to Step 5 | --

5

1. Turn the ignition switch to the OFF position.
2. Reconnect all connectors/components removed.

Have all the repairs been made?

--

Go to Power Windows System Check

--

## Power Window Inoperative - Right Side Front from both window switches

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the entire power windows system check performed? | -- | Go to Step 2 | Go to Power Windows System Check

2

1. Place the ignition switch into the OFF position.
2. Disconnect the RF window switch.
3. Place the ignition switch into the RUN position.
4. Using a test light, backprobe the RF window switch connector from terminals H and D.
5. Press the LF window switch to the UP and DOWN positions.

Does the test light illuminate in both cases?

--

Go to Step 3

Go to Step 4

3

1. Turn the ignition switch to the OFF position.
2. Disconnect the RF window regulator motor.
3. Check for a short to ground and continuity in CKT 666 and 667.

Are either of these conditions present?

--

Go to Step 5

Go to Step 6

4

1. Using a test light, backprobe the LF window switch connector from terminals B and F.
2. Press the LF window switch to the UP and DOWN positions.

Does the test light illuminate in both cases?

--

Go to Step 7

Go to Step 8

5

1. Reconnect the RF window switch.
2. Place the ignition switch into the RUN position.
3. Using a test light, backprobe the RF window switch connector from terminals A and E.
4. Press the RF window switch to the UP and DOWN positions.

Does the test light illuminate in both cases?

--

Go to Step 9

Go to Step 10

6 | Repair the open or short to ground in CKT 666 or 667. Is the repair complete? | -- | Go to Step 11 | --
7 | Repair the open in CKT 166 or 167. Is the repair complete? | -- | Go to Step 11 | --
8 | Replace the LF window switch. Refer to Door Trim Plate Replacement . Is the repair complete? | -- | Go to Step 11 | --
9 | Replace the RF window regulator motor. Refer to Front Side Door Window Regulator Replacement . Is the repair complete? | -- | Go to Step 11 | --
10 | Replace the RF window switch. Refer to Door Trim Plate Replacement . Is the repair complete? | -- | Go to Step 11 | --

11

1. Turn the ignition switch to the OFF position.
2. Reconnect all connectors/components removed.

Have all the repairs been made?

--

Go to Power Windows System Check

--