Power Door Locks Actuator Motor Inoperative. Opel Sintra 1999

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---

1

1. Disconnect inoperative door lock actuator motor electrical connector.
2. Connect a test lamp between the inoperative door lock harness connector terminals A an B.
3. Verify that the sliding door(s) are closed when diagnosing an actuator motor on a sliding door.
4. While observing the test lamp, press either door lock switch to the UNLOCK position.

Does the test lamp flash once upon pressing UNLOCK?

--

Go to Step 3

Go to Step 2

2

1. Connect a test lamp between inoperative door lock harness connector terminal A (terminal B on sliding door) and ground.
2. While observing the test lamp, press either door lock switch to the UNLOCK position.

Does the test lamp flash once upon pressing UNLOCK?

--

Go to Step 4

Go to Step 5

3 | Replace the inoperative door lock actuator motor. Refer to Front Side Door Lock Actuator Replacement . Is the repair complete? | -- | Go to Automatic Door Locks System Check | --

4

• | Check door lock switch plate plungers and striker for good connection.

• | If OK, repair poor connection or open in circuit 295.

Is the repair complete?

--

Go to Automatic Door Locks System Check

--

5

Repair poor connection or open in:

• | Driver's door lock: circuit 694.

• | Passenger door locks: circuit 294.

• | When diagnosing sliding doors actuator motors, check door lock switch plate plungers and striker for good connection.

Is the repair complete?

--

Go to Automatic Door Locks System Check

--