Contact Plate Replacement - Sliding Door. Opel Sintra 1999

For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 38778 Door Trim Pad and Garnish Clip Removal

1. Open the power sliding door.
2. Use the J 38778 in order to unsnap the door mounted plunger push-in retainers from the sliding door.
3. Remove the door mounted plungers from the sliding door.
4. Disconnect the electrical connector from the door mounted plungers.

### Installation Procedure

1. Connect the electrical connector to the door mounted plungers.
2. Install the door mounted plungers to the sliding door.
3. Install the push-in retainers in order to secure the door mounted plungers to the sliding door.
4. Close the power sliding door.