Engine Oil Level Switch. Opel Sintra 1997

For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle.
2. Drain the engine oil.
3. Disconnect the electrical connector from Engine Oil Level Switch.
4. Remove the Engine Oil Level Switch from the oil pan.

### Installation Procedure

1. Install the Engine Oil Level Switch.

Tighten
Torque the Engine Oil Level Switch to 17-27 N·m (13-20 lb. ft.).

2. Lower the vehicle.
3. Add the engine oil to the correct level. For the crankcase oil capacity, refer to General Information.