Rotor/Drum Imbalance. Opel Sintra 1999

For 1990-2009 cars

Rotors and drums do not have a set tolerance. However, rotors or drums with more than 21 g (0.75 ounce) imbalance have the potential to cause vibration. Inspect the rotors and the drums for imbalance using either the on-vehicle or the off-vehicle method.

### Checking Rotor/Drum Imbalance (On-Vehicle)

1. Raise and suitable support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the tire and wheel assemblies.

• | For vehicles with steel wheels, refer to Tire and Wheel Removal and Installation in Tires and Wheels.

• | For Chevrolet and Oldsmobile vehicles with aluminum wheels, refer to Tire and Wheel Removal and Installation in Tires and Wheels.

• | For Pontiac vehicles with aluminum wheels, refer to Tire and Wheel Removal and Installation in Tires and Wheels.

Caution: One or more of the following guidelines may apply when performing specific required tests in the work stall:

• | When a test requires spinning the drive wheels with the vehicle jacked up, adhere to the following precautions:

- | Do not exceed 56 km/h (35 mph) when spinning one drive wheel with the other drive wheel stopped. This limit is necessary because the speedometer indicates only one-half the actual vehicle speed under these conditions. Personal injury may result from excessive wheel spinning.

- | If all of the drive wheels are spinning at the same speed, do not exceed 112 km/h (70 mph). Personal injury may result from excessive wheel spinning.

- | All persons should stay clear of the rotating components and the balance weight areas in order to avoid possible personal injury.

- | When running an engine in the repair stall for an extended period of time, use care not to overheat the engine and the transmission.

• | When a test requires jacking up the vehicle and running with the wheels and brake rotors removed, adhere to the following precautions:

- | Support the suspension at normal ride height.

- | Do not apply the brake with the brake rotors removed.

- | Do not place the transmission in PARK with the drive axles spinning.

- | Turn Off the ignition in order to stop the powertrain components from spinning.

• | When running an engine in the work stall, use the exhaust removal system to prevent breathing dangerous gases.

3. Reinstall the wheel nuts in order to retain the rotors/drums.
4. Run the vehicle at the complaint speed while inspecting for the vibration.
5. If the vibration still exists, perform the following steps:

5.1. | Remove the rotors/drums.

5.2. | Run the vehicle back to speed.

6. If the vibration is eliminated, perform the following steps:

6.1. | Remove the rotors/drums one at a time.

6.2. | Perform the vibration test for each rotor/drum.

6.3. | Replace the rotor/drum that is causing the imbalance.

6.4. | Inspect the balance of the new rotor/drum.

### Checking Rotor/Drum Imbalance (Off-Vehicle)

1. Measure the diameter and the width of the rotor/drum.
2. Mount the rotor/drum on a balancer in the same manner as a wheel.

Important: You can only inspect the rotors/drums for static imbalance. Ignore the dynamic imbalance reading.

3. Inspect for static imbalance.
4. If the rotor/drum shows imbalance, replace the rotor/drum.
5. Inspect the balance of the new rotor/drum before you install the rotor/drum on the vehicle.