Inline Harness Connector End Views. Opel Sintra 1999

For 1990-2009 cars

#### In-line Connector C101

Connector Part Information

• | 12160542

• | 20-Way F Micro-Pack 100 W Series Sealed (GRY)

Connector Part Information

• | 12193583

• | 20-Way M Micro-Pack 100 W Series Sealed (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | PPL | 1807 | Class 2 serial data communication | A | PPL | 1807 | Class 2 serial data communication
B | TAN | 800 | UART serial data communication | B | TAN | 800 | UART serial data communication
C | DK GRN | 35 | Coolant temperature indicator lamp output | C | DK GRN | 35 | Coolant temperature indicator lamp output
D | ORN/BLK | 434 | PARK/NEUTRAL input | D | ORN/BLK | 434 | PARK/NEUTRAL input
E | DK GRN/WHT | 762 | A/C request signal | E | DK GRN/WHT | 762 | A/C request signal
F | DK GRN | 890 | Fuel tank pressure sensor signal | F | DK GRN | 890 | Fuel tank pressure sensor signal
G | WHT | 1310 | Canister vent valve solenoid output | G | WHT | 1310 | Cannister vent valve solenoid output
H | DK BLU | 229 | Theft deterrent fuel enable signal | H | DK BLU | 229 | Theft deterrent fuel enable signal
J | BLK | 1057 | PCM sensor ground | J | BLK | 1057 | PCM sensor ground
K | PPL | 1589 | Fuel level sensor input | K | PPL | 1589 | Fuel level sensor input
L | ORN | 55 | Fuel level gauge sensor signal | L | ORN | 55 | Fuel level gauge sensor signal
M | GRY | 2700 | 5-volt reference | M | GRY | 2700 | 5-volt reference
N | LT GRN/BLK | 24 | Backup lamp feed | N | LT GRN/BLK | 24 | Backup lamp feed
P | BRN/WHT | 1173 | Low oil level indicator lamp output | P | BRN/WHT | 1173 | Low oil level indicator lamp output
R | ORN/BLK | 463 | TCS torque desired signal | R | ORN/BLK | 463 | TCS torque desired signal
S | DK GRN | 83 | Cruise control signal-disengage | S | DK GRN | 83 | Cruise control signal-disengage
T | WHT | 85 | Cruise control indicator lamp output | T | WHT | 85 | Cruise control indicator lamp output
U | BRN/WHT | 419 | Check engine indicator lamp output | U | BRN/WHT | 419 | Check engine indicator lamp output
V | PPL | 420 | Brake pedal switch output-torque converter clutch | V | PPL | 420 | Brake pedal switch output-torque converter clutch
W | TAN/BLK | 464 | TCS torque delivered signal | W | TAN/BLK | 464 | TCS torque delivered signal

#### In-line Connector C102

Connector Part Information

• | 12065425

• | 10-Way F Metri-Pack 150 Series Sealed (BLK)

Connector Part Information

• | 12048253

• | 10-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 1744 | Fuel injector 1 control | A | BLK | 1744f | Fuel injector 1 control
B | LT GRN/BLK | 1745 | Fuel injector 2 control | B | LT GRN/BLK | 1745 | Fuel injector 2 control
C | PNK/BLK | 1746 | Fuel injector 3 control | C | PNK/BLK | 1746 | Fuel injector 3 control
D | PNK | 639 | Fused ignition 1 feed | D | PNK | 639 | Fused ignition 1 feed
E | ORN/BLK | 469 | PCM sensor ground | E | ORN/BLK | 469 | MAP sensor return
F | GRY | 2704 | 7 volt reference signal | F | GRY | 416 | 7 volt reference signal
G | LT GRN | 432 | MAP sensor signal | G | LT GRN | 432 | MAP sensor signal
H | YEL/BLK | 846 | Fuel injector 6 control | H | YEL/BLK | 846 | Fuel injector 6 control
J | BLK/WHT | 845 | Fuel injector 5 control | J | BLK/WHT | 845 | Fuel injector 5 control
K | LT BLU/BLK | 844 | Fuel injector 4 control | K | LT BLU/BLK | 844 | Fuel injector 4 control

#### In-line Connector C103

Connector Part Information

• | 12052613

• | 2-Way F Metri-Pack 480 Series Sealed (BLK)

Connector Part Information

• | 12065863

• | 2-Way M Metri-Pack 480 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | YEL | 5 | Ignition switched battery feed-START | A | YEL | 5 | Ignition switched battery feed-START
B | RED | 102 | Fusible link battery feed | B | RED | 102 | Fusible link battery feed

#### In-line Connector C105

Connector Part Information

• | 12052613

• | 2-Way F Metri-Pack 480 Series Sealed (BLK)

Connector Part Information

• | 12186012

• | 2-Way M Metri-Pack 480 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | WHT | 504 | Ground | A | WHT | 504 | Ground
B | GRY | 532 | Engine coolant fan 2 (LH) feed | B | GRY | 532 | Engine coolant fan 2 (LH) feed

#### In-line Connector C108

Connector Part Information

• | 12110293

• | 3-Way F Metri-Pack 150 Series Sealed (BLK)

Connector Part Information

• | 12129615

• | 3-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 2761 | PCM sensor ground | A | BLK | 2761 | PCM sensor ground
B | YEL | 410 | Engine coolant temperature sensor signal | B | YEL | 410 | Engine coolant temperature sensor signal
C | DK GRN | 135 | Engine coolant temperature sensor | C | DK GRN | 135 | Engine coolant temperature sensor

#### In-line Connector C111

Connector Part Information

• | 12129508

• | 7-Way F Metri-Pack 150 (BLK)

Connector Part Information

• | 12146356

• | 7-Way F Metri-Pack 150 (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | LT GRN | 1222 | 1-2 shift solenoid valve control | A | LT GRN | 1222 | 1-2 shift solenoid valve control
B | YEL/BLK | 1223 | 2-3 shift solenoid valve control | B | YEL | 1223 | 2-3 shift solenoid valve control
C | BRN | 418 | TCC PWM SOL valve control | C | BLK | 418 | TCC PWM SOL valve control
D | TAN/BLK | 422 | TCC SOL valve control | D | TAN | 422 | TCC SOL valve control
E | PNK | 1339 | Fused ignition 1 feed | E | RED | 839 | Fused ignition 1 feed
F | YEL/BLK | 1227 | Transmission fluid temperature sensor signal | F | BRN | 1227 | Transmission fluid temperature sensor signal
G | ORN/BLK | 1057 | PCM sensor ground | G | GRY | 1057 | PCM sensor ground

#### In-line Connector C120

Connector Part Information

• | 12110293

• | 3-Way F Metri-Pack 150 Series Sealed (BLK)

Connector Part Information

• | 12129615

• | 3-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | LT GRN/BLK | 735 | Ambient air temperature sensor signal | A | LT GRN/BLK | 735 | Ambient air temperature sensor signal
B | BLK | 1550 | Ground | B | BLK | 1550 | Ground
C | DK BLU | 1393 | Courtesy lamps feed-protected battery | C | DK BLU | 1393 | Courtesy lamps feed-protected battery

#### In-line Connector C171

Connector Part Information

• | 12052641

• | 2-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12162000

• | 2-Way M Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 830 | LF wheel speed signal-high | A | LT BLU | 830 | LF wheel speed signal-high
B | WHT | 873 | LF wheel speed signal-low | B | YEL | 873 | LF wheel speed sensor-low

#### In-line Connector C172

Connector Part Information

• | 12052641

• | 2-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12162000

• | 2-Way M Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 833 | RF wheel speed signal-low | A | TAN | 833 | RF wheel speed signal-low
B | WHT | 872 | RF wheel speed signal-high | B | DK GRN | 872 | RF wheel speed signal-high

#### In-line Connector C181

Connector Part Information

• | 12160542

• | 20-Way F Micro-Pack Connector 100 W Series, Sealed (GRY)

Connector Part Information

• | 12160492

• | 20-Way M Micro-Pack Connector 100 W Series, Sealed (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | PPL | 1807 | Class 2 serial data communication | A | PPL | 1807 | Class 2 serial data communication
B | TAN | 800 | UART serial data communication | B | TAN | 800 | UART serial data communication
C | DK GRN | 35 | Coolant temperature indicator lamp output | C | DK GRN | 35 | Coolant temperature indicator lamp output
D | ORN/BLK | 434 | PARK/NEUTRAL input | D | ORN/BLK | 434 | PARK/NEUTRAL input
E | DK GRN/WHT | 762 | A/C request signal | E | DK GRN/WHT | 762 | A/C request signal
F | DK GRN | 890 | Fuel tank pressure sensor signal | F | DK GRN | 890 | Fuel tank pressure sensor signal
G | WHT | 1310 | Canister vent valve solenoid output | G | WHT | 1310 | Cannister vent valve solenoid output
H | DK BLU | 229 | Theft deterrent fuel enable signal | H | DK BLU | 229 | Theft deterrent fuel enable signal
J | ORN/BLK | 1057 | PCM sensor ground | J | ORN/BLK | 1057 | PCM sensor ground
K | PPL | 1589 | Fuel level sensor input | K | PPL | 1589 | Fuel level sensor input
L | ORN | 55 | Fuel level gauge sensor signal | L | ORN | 55 | Fuel level gauge sensor signal
M | GRY | 474 | 5-volt reference | M | GRY | 474 | 5-volt reference
N | LT GRN/BLK | 24 | Backup lamp feed | N | LT GRN/BLK | 24 | Backup lamp feed
P | BRN/WHT | 1173 | Low oil level indicator lamp output | P | BRN/WHT | 1173 | Low oil level indicator lamp output
R | ORN/BLK | 463 | Desired torque | R | ORN/BLK | 463 | Desired torque
S | DK GRN | 83 | Cruise control signal-disengage | S | DK GRN | 83 | Cruise control signal-disengage
T | WHT | 85 | Cruise control indicator lamp output | T | WHT | 85 | Cruise control indicator lamp output
U | BRN/WHT | 419 | Check engine indicator lamp output | U | BRN/WHT | 419 | Check engine indicator lamp output
V | PPL | 420 | Brake pedal switch output-torque converter clutch | V | PPL | 420 | Brake pedal switch output-torque converter clutch
W | TAN/BLK | 464 | Delivered torque | W | TAN/BLK | 464 | Delivered torque

#### In-line Connector C200

Connector Part Information

• | 12034257

• | 56-Way F Metri-Pack Mixed Series (BLK)

Connector Part Information

• | 12186339

• | 56-Way M Metri-Pack Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | ORN | 340 | Fused battery feed | A1 | ORN | 340 | Fused battery feed
A2 | LT BLU | 1894 | Power sliding door switch signal | A2 | LT BLU | 1894 | Power sliding door switch signal
A3-A6 | -- | -- | Not Used | A3-A6 | -- | -- | Not Used
A7 | GRY | 120 | Fuel pump motor feed | A7 | GRY | 120 | Fuel pump motor feed
A8 | BRN | 141 | Fused ignition 3 feed | A8 | BRN | 141 | Fused ignition 3 feed
A9 | BRN/WHT | 541 | Fused ignition 3 feed | A9 | BRN | 541 | Fused ignition 3 feed
B1 | -- | -- | Not Used | B1 | -- | -- | Not Used
B2 | LT GRN | 275 | Transaxle range switch feed-PARK | B2 | LT GRN | 275 | Transaxle range switch feed-PARK
B3 | GRY/BLK | 690 | Courtesy lamp control | B3 | GRY/BLK | 690 | Courtesy lamp control
B4 | ORN | 1240 | Fused battery feed | B4 | ORN | 1240 | Fused battery feed
B6-B7 | -- | -- | Not Used | B6-B7 | -- | -- | Not Used
B8 | DK BLU | 1393 | Courtesy lamps feed-protected battery | B8 | DK BLU | 1393 | Courtesy lamps feed-protected battery
B9 | -- | -- | Not Used | B9 | -- | -- | Not Used
C1 | PPL | 328 | Interior lamp override switch output | C1 | PPL | 328 | Interior lamp override switch output
C2 | YEL | 1139 | Fused ignition 1 feed | C2 | YEL | 1139 | Fused ignition 1 feed
C3 | BRN | 358 | Airbag indicator lamp output | C3 | BRN | 358 | Airbag indicator lamp output
C4 | ORN | 267 | Heated mirror element feed | C4 | ORN | 267 | Heated mirror element feed
C6 | LT GRN/BLK | 735 | Ambient air temperature sensor signal | C6 | LT GRN/BLK | 735 | Ambient air temperature sensor signal
C7 | DK GRN | 389 | Vehicle speed signal (VSS) | C7 | DK GRN | 389 | Vehicle speed signal (VSS)
C8 | -- | -- | Not Used | C8 | -- | -- | Not Used
C9 | PNK | 1039 | Fused ignition 1 feed | C9 | PNK | 1039 | Fused ignition 1 feed
D1-D2 | -- | -- | Not Used | D1-D2 | -- | -- | Not Used
D3 | BRN | 741 | Fused ignition 3 feed | D3 | BRN | 741 | Fused ignition 3 feed
D6 | ORN | 1140 | Fused battery feed | D6 | ORN | 1140 | Fused battery feed
D7-D8 | -- | -- | Not Used | D7-D8 | -- | -- | Not Used
E1 | -- | -- | Not Used | E1 | -- | -- | Not Used
E2 | TAN | 159 | Key in ignition output | E2 | TAN | 159 | Key in ignition output
E3 | DK BLU | 49 | Passenger door ajar switch signal | E3 | DK BLU | 49 | Passenger door ajar switch signal
E4-E6 | -- | -- | Not Used | E4-E6 | -- | -- | Not Used
E7 | BLK/WHT | 238 | Seat belt switch input | E7 | BLK/WHT | 238 | Seat belt switch input
E8-E9 | -- | -- | Not Used | E8-E9 | -- | -- | Not Used
F1 | TAN | 294 | Passenger door lock motor feed-unlock | F1 | TAN | 294 | Passenger door lock motor feed-unlock
F2 | GRY | 295 | Passenger door lock motor feed-lock | F2 | GRY | 295 | Passenger door lock motor feed-lock
F3 | ORN | 54 | Sliding door ajar signal battery | F3 | ORN | 54 | Sliding door ajar signal battery
F4 | -- | -- | Not Used | F4 | -- | -- | Not Used
F6 | ORN | 2540 | Fused battery feed | F6 | ORN | 2540 | Fused battery feed
F7 | PPL | 293 | Rear defogger element feed | F7 | PPL | 293 | Rear defogger element feed
F8-F9 | -- | -- | Not Used | F8-F9 | -- | -- | Not Used
G1 | -- | -- | Not Used | G1 | -- | -- | Not Used
G2 | LT BLU | 195 | Door lock switch input-battery | G2 | LT BLU | 195 | Door lock switch input battery
G3 | RED/BLK | 780 | Door lock-key cylinder | G3 | RED/BLK | 780 | Door lock-dey cylinder
G4 | ORN/BLK | 781 | Door unlock-key cylinder | G4 | ORN/BLK | 781 | Door unlock-key cylinder
G5 | -- | -- | Not Used | G5 | -- | -- | Not Used
G6 | TAN | 694 | Driver door unlock-battery | G6 | TAN | 694 | Driver door unlock-battery
G7 | WHT | 194 | Door unlock switch input-battery | G7 | WHT | 194 | Door unlock switch input-battery
G8-G10 | -- | -- | Not Used | G8-G10 | -- | -- | Not Used

#### In-line Connector C201

Connector Part Information

• | 12047842

• | 17-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12077822

• | 48-Way M Metri-Pack Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | -- | -- | Not Used | A1 | -- | -- | Not Used
A2 | PNK | 539 | Fused ignition 1 feed | A2 | PNK | 539 | Fused ignition 1 feed
A3 | -- | -- | Not Used | A3 | -- | -- | Not Used
A4 | PPL | 16 | Turn signal flasher output | A4 | PPL | 16 | Turn signal flasher output
A5 | -- | -- | Not Used | A5 | -- | -- | Not Used
A6 | DK BLU | 1415 | Turn signal lamp feed-right front | A6 | DK BLU/WHT | 1415 | Turn signal lamp feed-right front
A7 | LT BLU | 1414 | Turn signal lamp feed-left front | A7 | LT BLU/WHT | 1414 | Turn signal lamp feed-left front
A8-A10 | -- | -- | Not Used | A8-A10 | -- | -- | Not Used
A11 | BLK | 28 | Horn relay output-coil | A11 | BLK | 28 | Horn relay output-coil
A12 | GRY | 397 | Cruise ON/OFF signal | A12 | GRY | 397 | Cruise ON/OFF signal
A13 | PNK | 739 | Fused ignition 1 feed | A13 | PNK | 739 | Fused ignition 1 feed
A14 | DK BLU | 84 | Cruise control SET/COAST switch signal | A14 | DK BLU | 84 | Cruise control SET/COAST switch signal
A15 | GRY/BLK | 87 | Cruise control RESUME/ACCELERATE switch signal | A15 | GRY/BLK | 87 | Cruise control RESUME/ACCELERATE switch signal
A16 | BLK | 434 | PARK/NEUTRAL input | A16 | ORN/BLK | 434 | PARK/NEUTRAL input
A17 | DK GRN/WHT | 1135 | Stop lamp switched BTSI feed | A17 | DK GRN/WHT | 1135 | Stop lamp switched BTSI feed

#### In-line Connector C201

Connector Part Information

• | 12084183

• | 18-Way F Metri-Pack Mixed Series (BLK)

Connector Part Information

• | 12077822

• | 48-Way M Metri-Pack Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
B1 | -- | -- | Not Used | B1 | -- | -- | Not Used
B2 | BLK | 150 | Ground | B2 | BLK | 150 | Ground
B3 | LT GRN | 80 | Key in ignition input | B3 | LT GRN | 80 | Key in ignition input
B4 | TAN | 1559 | Ground | B4 | BLK | 1550 | Ground
B5-B6 | -- | -- | Not Used | B5-B6 | -- | -- | Not Used
C1 | WHT | 1390 | Ignition switched battery feed-ignition 0 | C1 | WHT | 1390 | Ignition switched battery feed-ignition 0
C2 | BLK | 150 | Ground | C2 | BLK | 150 | Ground
C3-C4 | -- | -- | Not Used | C3-C4 | -- | -- | Not Used
C5 | PNK | 3 | Ignition switched battery feed-ignition 1 | C5 | PNK | 3 | Ignition switched battery feed-ignition 1
C6 | ORN | 300 | Ignition switched battery feed-ignition 3 | C6 | ORN | 300 | Ignition switched battery feed-ignition 3
D1 | YEL | 5 | Ignition switched battery feed-START | D1 | YEL | 5 | Ignition switched battery feed-START
D2 | RED | 142 | Fused battery feed | D2 | RED | 142 | Fused battery feed
D3-D4 | -- | -- | Not Used | D3-D4 | -- | -- | Not Used
D5 | RED/WHT | 42 | Fused battery feed | D5 | RED | 42 | Fused battery feed
D6 | BRN | 4 | Ignition switched battery feed-accessory | D6 | BRN | 4 | Ignition switched battery feed-accessory

#### In-line Connector C201

Connector Part Information

• | 12047840

• | 13-Way F Metri-Pack 280 Series (LT-GRY)

Connector Part Information

• | 12077822

• | 48-Way M Metri-Pack Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
E1 | LT BLU | 1508 | Turn signal lamp/hazard lamp flasher feed | E1 | LT BLU | 1508 | Turn signal lamp/hazard lamp flasher feed
E2 | DK GRN | 113 | Windshield wiper switch signal-ON | E2 | DK GRN | 113 | Windshield wiper switch signal-ON
E3 | GRY | 112 | Windshield wiper switch signal-LOW/PULSE | E3 | GRY | 112 | Windshield wiper switch signal-LOW/Pulse
E4 | PPL | 92 | Windshield wiper motor feed-high speed | E4 | PPL | 92 | Windshield wiper motor feed-high speed
E5 | RED | 229 | Windshield washer pump motor feed | E5 | RED | 228 | Windshield washer pump motor feed
E6 | DK GRN | 19 | Tail/turn stop lamp feed-right rear | E6 | DK GRN | 19 | Tail/turn stop lamp feed-right rear
E7 | YEL | 18 | Tail/turn stop lamp feed-left rear | E7 | YEL | 18 | Tail/turn stop lamp feed-left rear
E8 | ORN | 1840 | Fused battery feed | E8 | ORN | 1840 | Fused battery feed
E9 | YEL/BLK | 243 | Fused accessory feed | E9 | YEL | 243 | Fused accessory feed
E10 | YEL/RED | 2340 | Fused battery feed | E10 | ORN | 2340 | Fused battery feed
E11 | LT GRN | 11 | High beam headlamp feed | E11 | LT GRN | 11 | High beam headlamp feed
E12 | TAN | 12 | Low beam headlamp feed | E12 | TAN | 12 | Low beam headlamp feed
E13 | YEL | 10 | Headlamp switch output | E13 | YEL | 10 | Headlamp switch output

#### In-line Connector C203

Connector Part Information

• | 12034257

• | 56-Way F Metri-Pack Mixed Series (BLK)

Connector Part Information

• | 12186339

• | 56-Way M Metri-Pack Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | ORN | 1052 | Auxiliary blower motor output | A1 | ORN | 1052 | Auxiliary blower motor output
A2 | YEL | 18 | Tail/turn/stop lamp feed-left rear | A2 | YEL | 18 | Tail/turn/stop lamp feed-left rear
A3 | DK GRN | 19 | Tail/turn/stop lamp feed-right rear | A3 | DK GRN | 19 | Tail/turn/stop lamp feed-right rear
A4 | LT BLU | 1134 | Park brake switch signal | A4 | LT BLU | 1134 | Park brake switch signal
A6 | -- | -- | Not Used | A6 | -- | -- | Not Used
A7 | GRY | 778 | Auxiliary blower motor switch output | A7 | GRY | 778 | Auxiliary blower motor switch output
A8 | WHT | 17 | Stop lamp switch output | A8 | WHT | 17 | Stop lamp switch output
A9 | YEL | 43 | Fused accessory feed | A9 | YEL | 43 | Fused accessory feed
B1 | -- | -- | Not Used | B1 | -- | -- | Not Used
B2 | GRY | 391 | Rear window wiper switch output | B2 | GRY | 391 | Rear window wiper switch output
B3 | BRN | 882 | RR wheel speed signal-high | B3 | BRN | 882 | RR wheel speed signal-high
B4 | WHT | 883 | RR wheel speed signal-low | B4 | WHT | 883 | RR wheel speed signal-low
B6 | BRN | 9 | Park lamp feed | B6 | BRN | 9 | Park lamp feed
B7 | WHT | 393 | Rear window wiper motor feed | B7 | WHT | 393 | Rear window wiper motor feed
B8 | DK GRN | 392 | Rear window washer pump motor feed | B8 | DK GRN | 392 | Rear window washer pump motor feed
B9 | -- | -- | Not Used | B9 | -- | -- | Not Used
C1 | BLK | 884 | LR wheel speed signal-high | C1 | BLK | 884 | LR wheel speed signal-high
C2 | RED | 885 | LR wheel speed signal-low | C2 | RED | 885 | LR wheel speed signal-low
C3 | LT BLU | 733 | Temperature valve position signal | C3 | LT BLU | 733 | Temperature valve position signal
C4 | -- | -- | Not Used | C4 | -- | -- | Not Used
C6 | YEL | 804 | Door ajar indicator lamp output | C6 | YEL | 804 | Door ajar indicator lamp output
C7 | TAN | 800 | UART serial data communication | C7 | TAN | 800 | UART serial data communication
C8 | PPL | 1589 | Fuel level sensor input | C8 | PPL | 1589 | Fuel level sensor input
C9 | -- | -- | Not Used | C9 | -- | -- | Not Used
D1 | LT BLU | 1072 | Auxiliary blower resistor output-medium | D1 | LT BLU | 1072 | Auxiliary blower resistor output medium
D2 | BLK/WHT | 351 | Ground-clean | D2 | BLK/WHT | 351 | Ground-clean
D3 | GRY | 8 | Interior lamp dim signal | D3 | GRY | 8 | Interior lamp dim signal
D6 | -- | -- | Not Used | D6 | -- | -- | Not Used
D7 | BLK | 1057 | PCM sensor ground | D7 | BLK | 1057 | PCM sensor ground
D8 | ORN | 640 | Fused battery feed | D8 | ORN | 640 | Fused battery feed
E1 | DK BLU | 46 | Speaker feed-right rear | E1 | DK BLU | 46 | Speaker feed-right rear
E2 | TAN | 201 | Speaker feed-left front | E2 | TAN | 201 | Speaker feed-left front
E3 | LT GRN | 200 | Speaker feed-right front | E3 | LT GRN | 200 | Speaker feed-right front
E4 | YEL | 116 | Speaker return-left rear | E4 | YEL | 116 | Speaker return-left rear
E6 | GRY | 474 | 5-volt reference | E6 | GRY | 474 | 5-volt reference
E7 | BLK | 906 | RSA enable out | E7 | BLK | 906 | RSA enable out
E8 | LT GRN | 1011 | RSA enable in | E8 | LT GRN | 1011 | RSA enable in
E9 | DK GRN | 890 | Fuel tank pressure sensor signal | E9 | DK GRN | 890 | Fuel tank pressure sensor signal
F1 | GRY/BLK | 308 | Park lamp switch output-park lamps ON | F1 | GRY/BLK | 308 | Park lamp switch output-park lamps ON
F2-F4 | -- | -- | Not Used | F2-F4 | -- | -- | Not Used
F6 | YEL | 1176 | Auxiliary blower resistor output-low | F6 | YEL | 1176 | Auxiliary blower resistor output-low
F7 | LT GRN/BLK | 24 | Backup lamp feed | F7 | LT GRN | 24 | Backup lamp feed
F8 | BLK | 1550 | Ground | F8 | BLK | 1550 | Ground
F9 | -- | -- | Not Used | F9 | -- | -- | Not Used
G1 | -- | -- | Not Used | G1 | -- | -- | Not Used
G2 | BRN | 641 | Fused ignition 3 feed | G2 | BRN | 641 | Fused ignition 3 feed
G3 | PNK | 39 | Fused ignition 1 feed | G3 | PNK | 39 | Fused ignition 1 feed
G4 | WHT | 1310 | Canister vent valve solenoid output | G4 | WHT | 1310 | Canister vent valve solenoid output
G5-G6 | -- | -- | Not Used | G5-G6 | -- | -- | Not Used
G7 | BRN | 199 | Speaker feed-left rear | G7 | BRN | 199 | Speaker feed-left rear
G8 | LT BLU | 115 | Speaker return-right rear | G8 | LT BLU | 115 | Speaker return-right rear
G9 | DK GRN | 117 | Speaker return-right front | G9 | DK GRN | 117 | Speaker return-right front
G10 | GRY | 118 | Speaker return-left front | G10 | GRY | 118 | Speaker return-left front

#### In-line Connector C205

Connector Part Information

• | 12092162

• | 4-Way F Metri-Pack 280 Series Sealed (GRY)

Connector Part Information

• | 12162477

• | 4-Way M Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | YEL | 443 | Fused accessory feed | A | YEL | 443 | Fused accessory feed
B | GRY | 1244 | Fused I/P dim signal | B | BRN | 1244 | Fused I/P dim signal
C | LT GRN | 1796 | Radio control signal-steering column | C | DK BLU | 1796 | Radio control signal-steering column
D | BLK | 1450 | Ground | D | BLK | 1450 | Ground

#### In-line Connector C215

Connector Part Information

• | 12092865

• | 2-Way F Metri-Pack 280 Series (YEL)

Connector Part Information

• | 12110149

• | 2-Way M Metri-Pack 280 Series (YEL)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | WHT | 347 | SIR inflator feed-driver | A | WHT | 347 | SIR inflator feed-driver
B | DK GRN | 348 | SIR inflator output-driver | B | DK GRN | 348 | SIR inflator output-driver

#### In-line Connector C216

Connector Part Information

• | 12077921

• | 2-Way F Metri-Pack 280 Series (YEL)

Connector Part Information

• | 12110288

• | 2-Way M Metri-Pack 280 Series (YEL)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | WHT/BLK | 1403 | Passenger inflator-high | A | WHT/BLK | 1403 | Passenger inflator-high
B | DK GRN/WHT | 1404 | Passenger inflator-low | B | DK GRN/WHT | 1404 | Passenger inflator-low

#### In-line Connector C301

Connector Part Information

• | 12064769

• | 10-Way F Metri-Pack 150 Series (NAT)

Connector Part Information

• | 12064770

• | 10-Way M Metri-Pack 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | WHT | 194 | Door unlock switch input-battery | A | WHT | 194 | Door unlock switch input-battery
B | TAN | 694 | Driver door unlock-battery | B | TAN | 694 | Driver door unlock-battery
C | LT BLU | 195 | Door lock switch input-battery | C | LT BLU | 195 | Door lock switch input-battery
D-K | -- | -- | Not Used | D-K | -- | -- | Not Used

#### In-line Connector C302

Connector Part Information

• | 12129430

• | 16-Way F ACT 280 Series (WHT)

Connector Part Information

• | 12129429

• | 16-Way M ACT 280 Series (WHT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 750 | Ground | A | BLK | 750 | Ground
B | DK GRN | 117 | Speaker return-right front | B | DK GRN | 117 | Speaker return-right front
C | LT GRN | 200 | Speaker feed-right front | C | LT GRN | 200 | Speaker fee-right front
D | -- | -- | Not Used | D | -- | -- | Not Used
E | BRN | 141 | Fused ignition 3 feed | E | BRN | 141 | Fused ignition 3 feed
F | LT BLU | 166 | LH front window switch feed-RH front window UP | F | LT BLU | 166 | LH front window switch feed-RH front window UP
G | DK BLU | 49 | Passenger door ajar switch signal | G | DK BLU | 49 | Passenger door ajar switch signal
H | YEL | 804 | Door ajar indicator lamp output | H | YEL | 804 | Door ajar indicator lamp output
J | GRY | 8 | Interior lamp dim signal | J | GRY | 8 | Interior lamp dim signal
K | TAN | 167 | LH front window switch feed-RH front window DOWN | K | TAN | 167 | LH front window switch feed-RH front window DOWN
L | RED/BLK | 780 | Door lock-key cylinder | L | RED/BLK | 780 | Door lock-key cylinder
M | ORN/BLK | 781 | Door unlock-key cylinder | M | ORN/BLK | 781 | Door unlock-key cylinder
N | RED/WHT | 881 | RH outside rearview mirror right/left feed | N | RED/WHT | 881 | RH outside rearview mirror right/left feed
P | LT BLU/WHT | 1497 | RH outside rearview mirror motor pack common feed | P | LT BLU/WHT | 1497 | RH outside rearview mirror motor pack common feed
R | BRN/WHT | 1498 | RH outside rearview mirror UP/DOWN feed | R | BRN/WHT | 1498 | RH outside rearview mirror UP/DOWN feed
S | GRY | 295 | Passenger door lock motor feed-lock | S | GRY | 295 | Passenger door lock motor feed-lock

#### In-line Connector C303

Connector Part Information

• | 12129430

• | 16-Way F ACT 280 Series (WHT)

Connector Part Information

• | 12129429

• | 16-Way M ACT 280 Series (WHT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 750 | Ground | A | BLK | 750 | Ground
B | GRY | 118 | Speaker return-left front | B | GRY | 118 | Speaker return-left front
C | TAN | 201 | Speaker feed-left front | C | TAN | 201 | Speaker feed-left front
D | ORN | 1140 | Fused battery feed | D | ORN | 1140 | Fused battery feed
E | BRN | 141 | Fused ignition 3 feed | E | BRN | 141 | Fused ignition 3 feed
F | LT BLU | 166 | LH front window switch feed-RH front window UP | F | LT BLU | 166 | LH front window switch feed-RH front window UP
G | TAN | 159 | Key in ignition output | G | TAN | 159 | Key in ignition output
H | YEL | 804 | Door ajar indicator lamp output | H | YEL | 804 | Door ajar indicator lamp output
J | GRY | 8 | Interior lamp dim signal | J | GRY | 8 | Interior lamp dim signal
K | TAN | 167 | LH front window switch feed-RH front window DOWN | K | TAN | 167 | LH front window switch feed-RH front window DOWN
L | RED/BLK | 780 | Door lock-key cylinder | L | RED/BLK | 780 | Door lock-key cylinder
M | ORN/BLK | 781 | Door unlock-key cylinder | M | ORN/BLK | 781 | Door unlock-key cylinder
N | RED/WHT | 881 | RH outside rearview mirror right/left feed | N | RED/WHT | 881 | RH outside rearview mirror right/left feed
P | LT BLU/WHT | 1497 | RH outside rearview mirror motor pack common feed | P | LT BLU/WHT | 1497 | RH outside rearview mirror motor pack common feed
R | BRN/WHT | 1498 | RH outside rearview mirror UP/DOWN feed | R | BRN/WHT | 1498 | RH outside rearview mirror UP/DOWN feed
S | GRY | 295 | Passenger door lock motor feed-lock | S | GRY | 295 | Passenger door lock motor feed-lock

#### In-line Connector C304

Connector Part Information

• | 12064769

• | 10-Way F Metri-Pack 150 Series (NAT)

Connector Part Information

• | 12064770

• | 10-Way M Metri-Pack 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | WHT | 194 | Door unlock switch input-battery | A | WHT | 194 | Door unlock switch input-battery
B | TAN | 294 | Passenger door lock motor feed-unlock | B | TAN | 294 | Passenger door lock motor feed-unlock
C | LT BLU | 195 | Door lock switch input-battery | C | LT BLU | 195 | Door lock switch input-battery
D-K | -- | -- | Not Used | D-K | -- | -- | Not Used

#### In-line Connector C305

Connector Part Information

• | 12146439

• | 4-Way F Metri-Pack 150 Series Sealed (GRY)

Connector Part Information

• | 15317612

• | 12-Way M Metri-Pack 280 Series Sealed (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1A | BRN | 882 | RR wheel speed signal-high | 1A | BRN | 882 | RR wheel speed signal-high
1B | WHT | 883 | RR wheel speed signal-low | 1B | WHT | 883 | RR wheel speed signal-low
1C | BLK | 884 | LR wheel speed signal-high | 1C | BLK | 884 | LR wheel speed signal-high
1D | RED | 885 | LR wheel speed signal-low | 1D | RED | 885 | LR wheel speed signal-low

#### In-line Connector C305

Connector Part Information

• | 12176335

• | 8-Way F Metri-Pack 280 Flexlock Series Sealed (NAT)

Connector Part Information

• | 15317612

• | 12-Way M Metri-Pack Mixed Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
3A | BLK | 250 | Ground | 3A | BLK | 250 | Ground
3B | BLK/WHT | 1057 | Ground-clean | 3B | ORN/BLK | 1057 | Ground-clean
3C | GRY | 120 | Fuel pump motor feed | 3C | GRY | 120 | Fuel pump motor feed
3D | PPL | 1589 | Fuel level sensor input | 3D | PPL | 1589 | Fuel level sensor input
3E | DK GRN | 890 | Fuel tank pressure sensor signal | 3E | DK GRN | 890 | Fuel tank pressure sensor signal
3F | WHT | 1310 | Canister vent valve solenoid output | 3F | WHT | 1310 | Canister vent valve solenoid output
3G | PNK | 1039 | Fused ignition 1 feed | 3G | PNK | 1039 | Fused ignition 1 feed
3H | GRY/BLK | 474 | 5-volt reference | 3H | GRY/BLK | 474 | 5-volt reference

#### In-line Connector C306

Connector Part Information

• | 12052641

• | 2-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12162000 (SWB)

• | 12186216 (LWB)

• | 2-Way M Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 882 | RR wheel speed signal-high | A | BRN | 882 | RR wheel speed signal-high
B | WHT | 883 | RR wheel speed signal-low | B | WHT | 883 | RR wheel speed signal-low

#### In-line Connector C308

Connector Part Information

• | 12092249

• | 23-Way F ACT 280 Series (BLK)

Connector Part Information

• | 12092248

• | 23-Way M ACT 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 901 | Rear quarter window switch-close | A | BLK | 901 | Rear quarter window switch-close
B | LT GRN/BLK | 735 | Ambient air temperature sensor signal | B | LT GRN/BLK | 735 | Ambient air temperature sensor signal
C | DK GRN | 389 | Vehicle speed signal | C | DK GRN | 389 | Vehicle speed signal
D | -- | -- | Update | D | YEL | 136 | Fuel level input
E | BLK/WHT | 1896 | Power sliding door system switch signal | E | BLK/WHT | 1896 | Power sliding door system switch signal
F | TAN | 800 | UART serial data communication | F | TAN | 800 | UART serial data communication
G | GRY | 8 | Interior lamp dim signal | G | GRY | 8 | Interior lamp dim signal
H | YEL | 43 | Fused accessory feed | H | YEL | 43 | Fused accessory feed
J | BLK | 1550 | Ground | J | BLK | 1550 | Ground
K | BRN | 741 | Fused ignition 3 feed | K | BRN | 741 | Fused ignition 3 feed
L | -- | -- | Not Used | L | -- | -- | Not Used
M | GRY/BLK | 308 | Park lamp switch output-park lamps ON | M | GRY/BLK | 308 | Park lamp switch output-park lamps ON
N | ORN | 640 | Fused battery feed | N | ORN | 640 | Fused battery feed
P | -- | -- | Not Used | P | -- | -- | Not Used
R | LT GRN | 24 | Backup lamp feed | R | -- | -- | Update
S | GRY/BLK | 690 | Courtesy lamp control | S | GRY/BLK | 690 | Courtesy lamp control
T | -- | -- | Not Used | T | -- | -- | Not Used
U | LT BLU | 1894 | Power sliding door switch signal | U | LT BLU | 1894 | Power sliding door switch signal
V | -- | -- | Not Used | V | -- | -- | Not Used
W | DK BLU | 1393 | Courtesy lamps feed-protected battery | W | DK BLU | 1393 | Courtesy lamps feed-protected battery
X | PPL | 328 | Interior lamp override switch output | X | PPL | 328 | Interior lamp override switch output
Y | BRN | 541 | Fused ignition 3 feed | Y | BRN | 541 | Fused ignition 3 feed
Z | BRN | 902 | Rear quarter window switch-open | Z | BLK | 902 | Rear quarter window switch-open

#### In-line Connector C309

Connector Part Information

• | 12052641

• | 2-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12162000 (SWB)

• | 12186216 (LWB)

• | 2-Way M Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 884 | LR wheel speed signal-high | A | BLK | 884 | LR wheel speed signal-high
B | WHT | 885 | LR wheel speed sensor-low | B | RED | 885 | LR wheel speed sensor-low

#### In-line Connector C313

Connector Part Information

• | 12064749

• | 2-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12064750

• | 2-Way M Metri-Pack 480 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN/BLK | 340 | Fused battery feed | A | ORN | 340 | Fused battery feed
B | BLK | 550 | Ground | B | BLK | 550 | Ground

#### In-line Connector C314

Connector Part Information

• | 12064749

• | 2-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12064750

• | 2-Way M Metri-Pack 480 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN/BLK | 340 | Fused battery feed | A | ORN | 340 | Fused battery feed
B | BLK | 550 | Ground | B | BLK | 550 | Ground

#### In-line Connector C400

Connector Part Information

• | 12015199

• | 2-Way F Metri-Pack 280 Series (NAT)

Connector Part Information

• | 12015271

• | 2-Way M Metri-Pack 280 Series Sealed (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 450 | Ground | A | BLK | 450 | Ground
B | PPL | 293 | Rear defogger element feed | B | PPL | 293 | Rear defogger element feed

#### In-line Connector C401

Connector Part Information

• | 12047785

• | 4-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12047786

• | 4-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | RED/BLK | 780 | Door lock-key cylinder | A | RED/BLK | 780 | Door lock-key cylinder
B | ORN/BLK | 781 | Door unlock-key cylinder | B | ORN/BLK | 781 | Door unlock-key cylinder
C | GRY | 391 | Rear window wiper switch output | C | GRY | 391 | Rear window wiper switch output
D | DK GRN | 392 | Rear window washer pump motor feed | D | DK GRN | 392 | Rear window washer pump motor feed

#### In-line Connector C402

Connector Part Information

• | 12047886

• | 8-Way F Metri-Pack 150 Flexlock Series Sealed (BLK)

Connector Part Information

• | 12045688

• | 8-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | YEL | 116 | Speaker return-left rear | A | YEL | 116 | Speaker return-left rear
B | BRN | 199 | Speaker feed-left rear | B | BRN | 199 | Speaker feed-left rear
C | BRN | 9 | Park lamp feed | C | BRN | 9 | Park lamp feed
D | WHT | 17 | Stop lamp switch output | D | WHT | 17 | Stop lamp switch output
E | YEL | 804 | Door ajar indicator lamp output | E | YEL | 804 | Door ajar indicator lamp output
F | DK BLU | 49 | Passenger door ajar switch signal | F | DK BLU | 49 | Passenger door ajar switch signal
G | DK BLU | 46 | Speaker feed-right rear | G | DK BLU | 46 | Speaker feed-right rear
H | LT BLU | 115 | Speaker return-right rear | H | LT BLU | 115 | Speaker return-right rear

#### In-line Connector C403

Connector Part Information

• | 12020397

• | 3-Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12020398

• | 3-Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | TAN | 294 | Passenger door lock motor feed-unlock | A | TAN | 294 | Passenger door lock motor feed-unlock
B | GRY | 295 | Passenger door lock motor feed-lock | B | GRY | 295 | Passenger door lock motor feed-lock
C | WHT | 393 | Rear window wiper motor feed | C | WHT | 393 | Rear window wiper motor feed

#### In-line Connector C405

Connector Part Information

• | 12064769

• | 10-Way F Metri-Pack 150 Series (NAT)

Connector Part Information

• | 12064770

• | 10-Way M Metri-Pack 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 1240 | Fused battery feed | A | ORN | 1240 | Fused battery feed
B | -- | -- | Not Used | B | -- | -- | Not Used
C | DK GRN | 19 | Tail/turn/stop lamp feed-right rear | C | DK GRN | 19 | Tail/turn/stop lamp feed-right rear
D | YEL | 18 | Tail/turn/stop lamp feed-left rear | D | YEL | 18 | Tail/turn/stop lamp feed-left rear
E | PNK | 39 | Fused ignition 1 feed | E | PNK | 39 | Fused ignition 1 feed
F | WHT | 17 | Stop lamp switch output | F | WHT | 17 | Stop lamp switch output
G | BRN | 9 | Park lamp feed | G | BRN | 9 | Park lamp feed
H | BLK | 1725 | Ground | H | BLK | 1725 | Ground
J-K | -- | -- | Not Used | J-K | -- | -- | Not Used

#### In-line Connector C407

Connector Part Information

• | 12052848

• | 6-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12124107

• | 6-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 1240 | Fused battery feed | A | ORN | 1240 | Fused battery feed
B | BRN | 9 | Park lamp feed | B | BRN | 9 | Park lamp feed
C | YEL | 18 | Tail/turn/stop lamp feed-left rear | C | YEL | 18 | Tail/turn/stop lamp feed-left rear
D | DK GRN | 19 | Tail/turn/stop lamp feed-right rear | D | DK GRN | 19 | Tail/turn/stop lamp feed-right rear
E | WHT | 17 | Stop lamp switch output | E | WHT | 17 | Stop lamp switch output
F | BLK | 1725 | Ground | F | BLK | 1725 | Ground