Quarter Window Replacement. Opel Sintra 1999

For 1990-2009 cars

## Quarter Window Replacement Front

### Removal Procedure

1. Remove the left body side front trim panel. Refer to Body Side Front Trim Panel Replacement - Left Side in Interior Trim.
2. Remove the body side rear upper trim panel. Refer to Third Pillar Trim Replacement in Interior Trim.
3. Remove the upper pillar trim panel. Refer to Center Pillar Upper Trim Panel Replacement in Interior Trim.
4. Remove the front quarter window latch screws.
5. Remove the front quarter window hinge stud nuts.
6. Remove the front quarter from the vehicle.

### Installation Procedure

1. Install the front quarter window to the vehicle.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the front quarter window hinge stud nuts.

Tighten
Tighten the nuts to 10 N·m (89 lb in).

3. Install the front quarter window latch screws.

Tighten
Tighten the screws to 8 N·m (70 lb in).

4. Remove the left body side front trim panel. Refer to Body Side Front Trim Panel Replacement - Left Side in Interior Trim.
5. Remove the body side rear upper trim panel. Refer to Third Pillar Trim Replacement in Interior Trim.
6. Install the upper pillar trim panel. Refer to Center Pillar Upper Trim Panel Replacement in Interior Trim.