Washers Inoperative. Opel Sintra 1999

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Wiper/Washer System Check performed? | -- | Go to Step 2 | Go to Wiper/Washer System Check
2 | Check the washer solvent container fluid level. Is the washer solvent container filled? | -- | Go to Step 4 | Go to Step 3
3 | Fill the washer solvent container. Is the washer solvent container filled? | -- | Go to Wiper/Washer System Check | --
4 | Check the hoses to ensure that they are correctly attached and that they are not pinched or kinked. Are the hoses OK? | -- | Go to Step 6 | Go to Step 5
5 | Repair the hoses. Is the repair complete? | -- | Go to Wiper/Washer System Check | --
6 | Check for clogged windshield washer nozzles. Are the nozzles clogged? | -- | Go to Step 7 | Go to Step 8
7 | Replace the clogged nozzles. Is the replacement complete? | -- | Go to Wiper/Washer System Check | --
8 | Check FRT WPR/WSHR fuse for an open fuse. Is the fuse open? | -- | Go to Step 9 | Go to Step 10
9 | Replace the open fuse. Is the replacement complete? | -- | Go to Wiper/Washer System Check | --

10

1. Disconnect the washer pump connector.
2. Turn the ignition switch to ON.
3. Connect a test light between terminals A and B of washer pump connector (harness side).
4. Activate the washer switch while observing the test light.

Is the test light on?

--

Go to Step 11

Go to Step 14

11 | Check for a poor connection at the washer pump connector. Is a poor connection present? | -- | Go to Step 12 | Go to Step 13
12 | Repair the poor connection. Is the repair complete? | -- | Go to Wiper/Washer System Check | --
13 | Replace the washer pump. Refer to Washer Pump Replacement . Is the replacement complete? | -- | Go to Wiper/Washer System Check | --

14

1. Connect the test light between the washer pump connector (harness side), terminal A, and ground.
2. Activate the washer switch while observing test light.

Is the test light on?

--

Go to Step 15

Go to Step 16

15 | Repair the poor connection condition or open circuit condition in CKT 1650. Is the repair complete? | -- | Go to Wiper/Washer System Check | --

16

1. Disconnect wiper/washer switch connector C201.
2. Connect the test light between wiper/washer connector C201, terminal E5, and ground.
3. Activate the washer switch.

Is the test light on?

--

Go to Step 17

Go to Step 18

17 | Repair the poor connection or open in CKT 228. Is the repair complete? | -- | Go to Wiper/Washer System Check | --
18 | Replace the wiper/washer switch. Refer to Multifunction, Turn Signal, and Hazard Switch Replacement - On Vehicle . Is the replacement complete? | -- | Go to Wiper/Washer System Check | --