WIDE OPEN THROT./A/C CUT-OUT SWITCH INTERFERENCE/1983 STE. Pontiac 6000 1983

For 1990-2009 cars

# WIDE OPEN THROT./A/C CUT-OUT SWITCH INTERFERENCE/1983 STE

SOME 1983 6000 STE VEHICLES BUILD BEFORE APRIL 15, 1983 MAY HAVE AN INTERFERENCE CONDITION BETWEEN THE LEFT-HAND HUSH PANEL AND THE WIDE OPEN THROTTLE COMPRESSOR CUT-OUT SWITCH. THE INTERFERENCE CONDITION PROHIBITS THE CYCLING OF THE SWITCH. THE CUSTOMER COMMENT COULD BE "LACK OF WIDE OPEN THROTTLE PERFORMANCE" ---TO CORRECT THE CONDITION, REMOVE THE LEFT SIDE HUSH PANEL. REMOVE THE INSULATION MATERIAL IN THE AREA WHERE HOLE IS TO BE MADE. USING A 1-3/8" HOLE SAW, REMOVE AREA SHOWN IN ILLUSTRATION. SEE ILLUSTRATION FOR WARRANTY INFORMATION

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.