LIGHTED VANITY MIRROR WIRING PINCHED. Pontiac 6000 1987

For 1990-2009 cars

# LIGHTED VANITY MIRROR WIRING PINCHED

LIGHTED VANITY MIRROR WIRE PINCHED BETWEEN INNER AND OUTER ROOF PANELS

#### MODELS AFFECTED 1987 6000 MODELS ---------------

#### Condition:

---------- The wire to the lighted visor vanity mirror may have excess length, which may be trapped between the inner and outer roof panels (see Illustration). The trapped wire may then be pinched or cut by the visor mounting screws. This then blows the 20 amp courtesy fuse.

#### Correction:

----------- 1. Disconnect negative battery cable.

2. Remove visor.

3. Remove garnish molding, and any other trim necessary, then pull down inner roof panel to gain access to wiring.

4. Repair wiring as necessary. Tape wire out of the way of the visor mounting holes.

5. Reinstall inner roof panel, and moldings previously removed.

6. Reinstall visor.

7. Reconnect negative battery cable.

#### Warranty Information:

Use existing labor operations.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.