UPDATE-REAR WHEEL ALIGNMENT SPECIFICATION. Pontiac 6000 1990

For 1990-2009 cars

# UPDATE-REAR WHEEL ALIGNMENT SPECIFICATION

#### Models Affected: 1990 6000 AWD (PAGE 6 REVISED)

Use the following rear wheel alignment specifications when checking or setting rear wheel alignment. Disregard any rear wheel alignment specifications for AWD in the 1990 Pontiac Service Manual.

Rear Sum Toe 0.2 0.2 (LH plus RH)

Rear Thrust Angle 0 0.15

Rear Camber 0.4 0.4

Rear Cross Camber 0 0.6 (LH plus RH)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.