WHEEL ALIGNMENT SPECIFICATION CORRECTION. Pontiac 6000 1982

For 1990-2009 cars

# WHEEL ALIGNMENT SPECIFICATION CORRECTION

Please revise the toe-in specification shown in the chart on Page 3A-3, Section 3A, of the 1982 Phoenix/6000 Service Manual as shown.

Make a note of this change in your copy of the Service Manual.

#### Wheel Alignment Specifications

Specifications for Diagnosis To Align for Warranty Repairs or Customer Paid Service

Camber ** 0 DEG +/- .50 DEG

mm (Per Wheel) 0 mm +/- 0.5 mm Toe-in DEG (Per Wheel) 0 DEG +/- .50 DEG

** Left and right side to be equal within .50 DEG.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.