CHOKE LIGHT INOPERATIVE WIRE MISINDEXED. Pontiac 6000 1986

For 1990-2009 cars

# CHOKE LIGHT INOPERATIVE WIRE MISINDEXED

#### VEHICLES AFFECTED: 1986 Pontiac 6000 with LE2 2.8L V-6 Engine and U52 Electronic Instrument Cluster Condition: ---------- The choke light is inoperative on 1986 Pontiac 6000's with LE2 2.8L V-6 engine and U52 electronic instrument cluster. Only cars built at Oshawa (VIN Code 9), before VIN 2G2AG19X3G9273606, are affected.

#### Cause:

Choke light wire misindexed in I.P. cluster connector no. 2.

#### Correction:

1. Disconnect negative battery cable.

2. Remove I.P cluster by: a. Remove left and centre lower trim plates. b. Remove centre trim pad. c. Remove cluster.

3. Unsnap connector no. 2 from I.P. (black connector). Pull connector out for access. Remove terminal from cavity no. 8 of connector (light blue wire) and reinstall in cavity no. 11. See page 8A-82-7 or 1986 Pontiac 6000 Service Manual for view of connector.

4. Note this change on pages 8A-82-7, and 8A-82-0 of your Service Manual.

5. Reinstall I.P. cluster.

6. Reconnect negative battery cable.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.