SERVICE GUILD: CROSS-GROOVE DESIGN CONSTANT VELOCITY AXLE. Pontiac 6000 1988

For 1990-2009 cars

# SERVICE GUILD: CROSS-GROOVE DESIGN CONSTANT VELOCITY AXLE

CROSS-GROVE DESIGN CONSTANT-VELOCITY (CV) JOINT

#### Models Affected 1988 SUNBIRD 2.OL Turbo LT3 (VIN M) ---------------- 5 SP Manual MG2 1988 GRAND AM 2.3L MPFI LD2 (VIN D) Quad 4 5 SP Manual MG2 1988 6000 2.8L MPFI LB6 (VIN W) 5 SP Manual MG2

Certain 1988 Sunbird, Grand Am and 6000 models with performance oriented combinations of engine, transaxle and suspension options use a new cross- grove design constant-velocity (CV) joint at the inboard(transaxle) end of the drive axle assembly. The joint can be identified by the cylindrical shape of its outer housing. Refer to the figure for the proper seal collapse dimension when making repairs to the seal, clamps, or housing assembly.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.