POSSIBLE POWER MIRROR SWITCH- DAMAGE-DISCONNECT BATTERY. Pontiac 6000 1986

For 1990-2009 cars

# POSSIBLE POWER MIRROR SWITCH- DAMAGE-DISCONNECT BATTERY

TO PREVENT POSSIBLE DAMAGE TO THE POWER MIRROR SWITCH, DISCONNECT THE NEGATIVE CABLE FROM BATTERY POST BEFORE DISCONNECTING OR CONNECTING THE POWER MIRROR SWITCH CONNECTOR.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.