AIR CONDITIONING ORIFICE TUBE RELOCATION. Pontiac 6000 1986

For 1990-2009 cars

# AIR CONDITIONING ORIFICE TUBE RELOCATION

1986 6000 MODELS

On 1986 6000 models, the air conditioning orifice tube was moved from the inlet of the evaporator to the connection at the condensor (refer to Figure 1). The orifice tube was relocated to eliminate the hissing sound which was objectionable to some owners.

Some technicians have not been aware of this relocation and have installed another orifice tube back at the evaporator. This obviously will severely reduce cooling. To check for the orifice tube by the condensor, feel the liquid line, it should be cold when the air conditioning is in operation.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.