LUGGAGE CARRIER NOISE INCORRECT INSTALLATION. Pontiac 6000 1984

For 1990-2009 cars

# LUGGAGE CARRIER NOISE INCORRECT INSTALLATION

#### VEHICLES AFFECTED: 1984 'A' Station Wagons

Some 1984 'A-35' wagons may experience a windnoise caused by the roof luggage carrier. Ensure that the existing cross members of the luggage carrier are installed correctly as per 1984 Product Service Bulletin 2-102. If the condition still persists the current cross rails may be replaced with the following parts:

Release Part No. Part Name -------- --------- 14086340 Cross Rail assembly - roof luggage carrier (bright) - 2 req'd per vehicle (Base A Car)

14086342 Cross Rail assembly - roof luggage carrier (black) - 2 req'd per vehicle (Celebrity Eurosport)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.