REWORK OF REAR COMPARTMENT LID HINGE ASSEMBLY. Pontiac 6000 1984

For 1990-2009 cars

# REWORK OF REAR COMPARTMENT LID HINGE ASSEMBLY

#### VEHICLES AFFECTED: ALL 1982 THROUGH 1987 A-19, 27 STYLES

If a new service hinge is required on a vehicle with optional rear seat shoulder belts. It may be necessary to cut notches to the outboard flanges of the service hinge assembly as shown in the attached illustration.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.