SERVICE MANUAL UPDATE (AWD 6000 STE) TOWING INFORMATION. Pontiac 6000 1988

For 1990-2009 cars

# SERVICE MANUAL UPDATE (AWD 6000 STE) TOWING INFORMATION

#### Models Affected: 1988-89 6000 STE

#### SERVICE MANUAL UPDATE

The following information is to be added to General Information Section page OA-7 of the Service Manual.

#### NOTICE: WHEN LIFTING, JACKING, OR SUPPORTING AN ALL WHEEL DRIVE (AWD) VEHICLE, BE CERTAIN THAT ONLY FRAME OR WHEEL CONTACT HOISTS, JACK, OR JACKSTANDS ARE USED.

DO NOT LIFT, JACK, OR SUPPORT AN AWD VEHICLE BY THE TRANSVERSE SPRING. LIFTING, JACKING, OR SUPPORTING AN AWD VEHICLE WITH SUSPENSION CONTACT EQUIPMENT MAY FRACTURE THE TRANSVERSE SPRING, AS THE EQUIPMENT CONTACTS THE SPRING. A FRACTURED TRANSVERSE SPRING CAN LEAD TO FAILURE OF THE SPRING.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.