NEW HYDRAULIC ENGINE MOUNTS CORRECT LOW SPEED RATTLE. Pontiac 6000 1985

For 1990-2009 cars

# NEW HYDRAULIC ENGINE MOUNTS CORRECT LOW SPEED RATTLE

1985 6000 WITH LB6, LE2, AND LR8 ENGINES

Some 1985 6000 vehicles may experience a rattle type noise from the engine compartment which may be caused by the hydraulic engine mount (see illustration). This condition may be corrected by the installation of a new mount.

To repair vehicles experiencing this condition, use the mounts as listed on the following chart:

COLOR NEW P/N CODE USAGE ------- ---- ----- 17983733 White Pontiac 6000 with LB6 and LE2 V6 Engine

17983732 Purple Pontiac 6000 with LR8 L4 Engine

The procedures to be followed for this repair are detailed in the appropriate section of the service manual. Use applicable labor operation number and labor times.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.