AUTO TRANSMISSION COOLER LINE CHAFING ON HORN ASSEMBLY. Pontiac 6000 1985

For 1990-2009 cars

# AUTO TRANSMISSION COOLER LINE CHAFING ON HORN ASSEMBLY

1985 6000 WITH LR8 2.5 ENGINE (VIN CODE R) AUTOMATIC TRANSMISSION AND DUAL HORNS

Some of the above vehicles may have the transmission cooler line (rubber hose) rubbing on the rear horn assembly at the front left hand side of the engine compartment.

This can be corrected by bending the metal portion of cooler line, above the rubber hose, inboard away from the horn to maintain a minimum clearance of 1/2 inch.

The cooler line hose should be inspected for abrasion and replaced if necessary.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.