ELECTRONIC LEVEL CONTROL OPERATION OF SYSTEM. Pontiac 6000 1982

For 1990-2009 cars

# ELECTRONIC LEVEL CONTROL OPERATION OF SYSTEM

The 6000 electronic ride control can automatically compensate for a load increase with the ignition switch in the "on" or "off" position. Operation of the compressor with the ignition in the "off" position is limited to five cumulative minutes each time the ignition has been turned off.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.