WINDOW REGULATOR HANDLE INSUFFICIENT CLEARANCE. Pontiac 6000 1982

For 1990-2009 cars

# WINDOW REGULATOR HANDLE INSUFFICIENT CLEARANCE

SOME 1982 "A" STYLES MAY EXHIBIT AN INTERFERENCE CONDITION BETWEEN THE DOOR WINDOW REGULATOR HANDLE PLATE AND THE DOOR TRIM PAD RESULTING IN EXCESSIVE DOOR WINDOW OPERATING EFFORTS. SHOULD THIS CONDITION OCCUR, THE FOLLOWING PROCEDURE SHOULD BE FOLLOWED: 1.USING A SUITABLE TOOL, REMOVE THE DOOR WINDOW REGULATOR HANDLE. 2.DISCARD THE ORIGINAL DOOR WINDOW REGULATOR HANDLE PLATE. 3.INSTALL THE PLASTIC BEARING PLATE, PART NO. 20375300. 4.INSTALL THE DOOR WINDOW REGULATOR HANDLE. ** ILLUSTRATION **

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.