INOP 'DOOR AJAR' WARNING LIGHT NEW 'DOOR AJAR' SWITCH. Pontiac 6000 1984

For 1990-2009 cars

# INOP 'DOOR AJAR' WARNING LIGHT NEW 'DOOR AJAR' SWITCH

#### VEHICLES AFFECTED: 1984 Pontiac 6000 'STE'

An intermittent or inoperative 'Door Ajar' light on the Driver Information Centre (D.I.C.) could be caused by an inoperative door ajar switch.

To verify the condition, depress the switch and observe the D.I.C. Any inoperative switch should be replaced with a new switch part number 20555200.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.