DIESEL FRONT CAMSHAFT BEARING INSTALLATION. Pontiac 6000 1982

For 1990-2009 cars

# DIESEL FRONT CAMSHAFT BEARING INSTALLATION

USE THE FOLLOWING PROCEDURE WHEN INSTALLING A FRONT CAMSHAFT BEARING AND RETAINER ASSEMBLY ON A 4.3L V-6 DIESEL ENGINE. 1.POSITION THE BEARING AND RETAINER ASSEMBLY ON THE BLOCK AND LOOSELY INSTALL THE BOLTS. 2.ROTATE THE CAMSHAFT AT LEAST FOUR (4) TURNS TO CENTER THE RETAINER 3.TORQUE CAMSHAFT BEARING RETAINER BOLTS EVENLY TO SPECIFICATIONS. 4.ROTATE THE CAMSHAFT TO BE SURE IT'S FREE. IF NOT, REPEAT THE PROCEDURE.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.