INOP 'DOOR AJAR' WARNING LIGHT NEW 'DOOR AJAR' SWITCH. Pontiac 6000 1983

For 1990-2009 cars

# INOP 'DOOR AJAR' WARNING LIGHT NEW 'DOOR AJAR' SWITCH

6000 STE

#### CONDITION:

---------- Intermittent or inoperative "Door Ajar" light on Driver Information Center (D.I.C.).

#### CAUSE:

------ Door ajar switch electrical contacts do not close or open properly.

#### CORRECTION:

-----------

1. Depress plunger and observe D.I.C. to verify condition.

2. Remove any inoperative door ajar switch or switches and disconnect wires.

3. Replace the inoperative switch(es) with new switch, part number 20555200.

4. Reconnect wires and install new switch into door pillar.

5. Open and close doors to verify proper operation.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.