DAMAGED/PIERCED A/C CONDENSER INSPECT VALANCE PANEL SCREWS. Pontiac 6000 1990

For 1990-2009 cars

# DAMAGED/PIERCED A/C CONDENSER INSPECT VALANCE PANEL SCREWS

#### Subject: DAMAGED A/C CONDENSER BY VALANCE PANEL SCREWS (REPLACE WITH SHORTER SCREWS)

#### Models Affected: 1990-91 6000 MODELS

#### Condition:

---------- The A/C condenser could be pierced at the bottom by the four (4) front center valance panel retaining screws.

#### Cause:

------- The four (4) center screws used to retain the front valance panel may be too long 20.0 Mm (13/16 inch). This causes the screws to pierce the condenser during jounce conditions.

#### Correction:

------------ Replace the four (4) valance panel retaining screws with the following shorter service part which is 15.0 to 16.0 mm (5/8 inch) long.

Quantity Part Number Part Name --------- ----------- ---------- 4 12337913 Screw

Parts are currently available from GMSPO.

The potential for this condition occurred some time during the 1990 production and carried over into the early 1991 production. There are no VIN breakpoints available.

The four (4) center valance panel screws should be replaced whenever a damaged A/C condenser is replaced.

Labor Operation Number: T1699 Labor Time : 1.8 Hours

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.