RACK & PINION 'SHORT GEAR' FOR REAR WHEEL-DRIVE VEHICLES. Pontiac Acadian (Canada) 1981

For 1990-2009 cars

# RACK & PINION 'SHORT GEAR' FOR REAR WHEEL-DRIVE VEHICLES

#### VEHICLES AFFECTED: 1981-85 'T' Series Vehicles 1984-85 Corvette

'Short gear' rack & pinion assemblies are available for service replacement. The short gear is a complete gear assembly except for the following:

1. Inner and outer tie rod assemblies

2. Tie rod boots.

3. Breather tube.

4. Attachment hardware.

Boot clamps are included with the short gear.

Use of the short gear is recommended when the expense of individual parts and required labour necessary to service a rack & pinion assembly would exceed the expense of installing the short gear assembly. The short gear incorporates all product improvements made since 1982.

Refer to the appropriate chassis service manual for information on parts transfer or R&R procedures.

#### REPLACEMENT APPLICATION

Service Short Labour Labour Year and Model Gear P/N Operation Time -------------- ------------- --------- ------

1981-85 'T' Series Vehicles 7846718 E9730 1.4

1984-85 Corvette 7846734 E9730 1.7

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.