ENGINE MISS DURING WARM-UP EFE RELAY CHATTER ERRONEOUS 44. Pontiac Acadian (Canada) 1981

For 1990-2009 cars

# ENGINE MISS DURING WARM-UP EFE RELAY CHATTER ERRONEOUS 44

A NEW SERVICE PROM HAS BEEN RELEASED TO ALLEVIATE SPECIFIC CUSTOMER COMMENTS SUCH AS ENGINE "MISS" DURING WARM-UP, EFE RELAY CHATTER AT WIDE OPEN THROTTLE, OR A CODE 44 SET AT HIGH SPEEDS (APPROXIMATELY 70 MPH), DURING NORMAL SYSTEM OPERATION. THE NEW CALIBRATION SERVICE PROM'S ARE: APPLICATION ALL MANUAL TRANSMISSION EXCEPT 1TJ08 AND C41 ECM PRODUCTION 16013891 NEW SERVICE PROM 1225967 APPLICATION MANUAL TRANSMISSION 1TJ08 AND C41 ECM PRODUCTION 16017661 NEW SERVICE PROM 1225968 APPLICATION ALL AUTOMATIC TRANSMISSION ECM PRODUCTION 16013931 NEW SERVICE PROM 1225969 THE CURRENT SERVICE PROM'S ARE SATISFACTORY FOR SERVICE OF UNITS WITH CONDITIONS OTHER THAN THOSE DESCRIBED ABOVE AND SHOULD BE USED UNTIL STOCK IS EXHAUSTED. USE APPLICABLE LABOR OPERATION.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.