UPDATE SHOP MANUAL; HOT PLUG, INJ. TIMING, & IDLE SPEED SPEC. Pontiac Acadian (Canada) 1984

For 1990-2009 cars

# UPDATE SHOP MANUAL; HOT PLUG, INJ. TIMING, & IDLE SPEED SPEC

#### VEHICLES AFFECTED: 1982-84 "T" Series

The following revisions should be noted in the subject Shop Manuals: Section 6A2, 1.8 Liter Diesel Engine and Section 6C3, Diesel Fuel Injection.

Page 6A2-13 Hot Plug Replacement specification should be 1000-1250 kg (2200-2760 lbs.)

Page 6A2-26 General Data and specifications

(1) Fuel injection timing B.T.D.C. (static) specification should be 18 DEG.

(2) Idle Speed specification should be A/T-725 M/T-625.

Page 6C3-5, Figures 6C3-12, 13 should be revised as shown in Figures 6C3-12A and 6C3-13A below.

Please make note of these changes to your copy of the 1982, 1983 and 1984 Pontiac Acadian and 1000 Shop Manuals and the Chevette Shop Manuals.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.