SPARK KNOCK NEW PROM INFORMATION. Pontiac Fiero 1984

For 1990-2009 cars

# SPARK KNOCK NEW PROM INFORMATION

1984 FIERO WITH 2.5L ENGINE AND MANUAL TRANSAXLE

A customer comment of spark knock on the 2.5L engine may be received. If normal diagnosis in Section 6E2 of the Service Manual does not repair this condition, a new PROM (P/N 1227134) may be installed. This applies only to Fiero models with manual transaxle.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.