LEFT HAND REAR DRIVE AXLE CV JOINT BOOT SPLITTING. Pontiac Fiero 1984

For 1990-2009 cars

# LEFT HAND REAR DRIVE AXLE CV JOINT BOOT SPLITTING

#### CONDITION:

SPLIT DRIVE AXLE BOOT. LOSS OF CV JOINT LUBRICATION AND/OR A CLUNKING SOUND EMITTING FROM LEFT HAND REAR AXLE AREA. CAUSE: LEFT HAND RUBBER SPLASH SHIELD MAY BE CONTACTING OUTER DRIVE AXLE CV JOINT BOOT. CORRECTION: USING TEMPLATE SUPPLIED, TRIM EXCESS MATERIAL FROM SPLASH SHIELD AND INSTALL NEW DRIVE AXLE BOOT. NOTICE: IF CV JOINT HAS BEEN DAMAGED BECAUSE LOSS OF LUBE, ENTIRE JOINT MUST BE REPLACED. PROCEDURE: A. HOIST VEHICLE. B. REMOVE LEFT REAR WHEEL. C. POSITION TEMPLATE ON SPLASH SHIELD AND TRIM ACCORDING TO TEMPLATE. WARRANTY INFORMATION LABOR OPERATION T-3138 TIME ALLOWANCE .4 HOURS TROUBLE CODE 62 FOR REPLACEMENT OF CV JOINT BOOK, USE APPLICABLE LABOR TIME.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.