REAR ALIGNMENT SPECIFICATION CHANGE. Pontiac Fiero 1984

For 1990-2009 cars

# REAR ALIGNMENT SPECIFICATION CHANGE

1984-87 FIERO MODELS

The rear suspension toe specification for the 1987 Fiero has changed from:

.15 Degree +/- .1 Degree (Per Wheel)

to 0 Degree +/- .1 Degree (Per Wheel)

This new specification is also applicable to 1984-86 Fiero models.

SERVICE DEPARTMENT PONTIAC DIVISION GENERAL MOTORS CORPORATION

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.