ENGINE REPLACEMENT LABOR OPERATIONS FIERO 2.5L. Pontiac Fiero 1984

For 1990-2009 cars

# ENGINE REPLACEMENT LABOR OPERATIONS FIERO 2.5L

1984-85 FIERO EQUIPPED WITH 2.5L ENGINE

The following Labor Operations have been revised, effective immediately. The new times are:

J1800 Block, Engine Fitted - Replace 8.6 hrs.

ADD : With A/C .9 hrs. With Cruise Control .1 hr.

J1820 Engine, Partial/Basic - Replace 7.7 hrs.

ADD : With A/C .9 hrs. With Cruise Control .1 hr.

J1880 Engine Assembly - Replace 4.9 hrs.

ADD : With A/C .9 hrs. With Cruise Control .1 hr.

All other times used in conjunction with these Labor Operations will remain the same.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.