REAR COMPARTMENT TORQUE ROD SERVICE MANUAL REVISION. Pontiac Fiero 1984

For 1990-2009 cars

# REAR COMPARTMENT TORQUE ROD SERVICE MANUAL REVISION

#### VEHICLES AFFECTED: 1984-87 P CAR

SHOP MANUAL UPDATE

The purpose of this bulletin is to advise of a revision to figure 7-3, rear compartment torque rods, shown in section 7J of all (1984-87) Fiero Service Manuals.

When adjusting or installing torque rod retaining pins, item 9, must be installed from the inboard side as shown in figure 1.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.