SAG IN DOOR TRIM PANEL INSTALL BRACKET BEHIND MIRROR. Pontiac Fiero 1985

For 1990-2009 cars

# SAG IN DOOR TRIM PANEL INSTALL BRACKET BEHIND MIRROR

#### Subject: FIERO DOOR TRIM PAD REPAIR,

1985 FIERO WITH MANUAL REMOTE T-SIDE REAR VIEW MIRROR

SOME 1985 FIEROS EQUIPPED WITH MANUAL REMOTE MIRROR MAY EXPERIENCE, A SAG IN THE DOOR TRIM PANEL AT THE REMOTE MIRROR CONTROL LOCATION. THIS CONDITION CAN BE CORRECTED BY ADDING A REINFORCEMENT TO THE BACK OF THE TRIM PANEL AS FOLLOWS:

1. REMOVE DOOR TRIM PANEL AND PLACE TRIM SIDE DOWN ON CLEAN WORK SURFACE.

2. FROM A PIECE OF ALUMINUM APPROXIMATELY .020-.025 THICK, CUT A SECTION TO FIT ACROSS THE SAG AREA ON THE TRIM PANEL.

3. USING 3M STRUCTURAL ADHESIVE, 8101 OR EOUIVALENT, BOND REINFORCEMENT TO THE TRIM PANEL, IT MAY BE NECESSARY TO CLAMP REINFORCEMENT FOR INITIAL SET-UP.

4. REINSTALL TRIM PAD.

LABOR OPERATION: T1173

LABOR TIME .8 HOURS

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.