CLEAR COAT LABOR AND MATERIAL ALLOWANCE CORRECTIONS-84 FIERO. Pontiac Fiero 1984

For 1990-2009 cars

# CLEAR COAT LABOR AND MATERIAL ALLOWANCE CORRECTIONS-84 FIERO

The April, 1984 revision of Labor Time Guide contains several errors affecting Clear Coat labor and material Allowances for the Fiero (P-series). The following is a list of corrections:

LABOR ADD: TO CLEAR COAT OPERATON NUMBER PUBLISHED 4/84 EFFECTIVE 5/84

A0339, A0347, A0357 1.1 .2 CH CD A0679, A0680, A0681 .6 .2 A0689, A0690, A0691 CC CB A0800, A0801, A0810, A0811 .3 .2 CA A0819, A0820, A0830 .8 .2 CF CC A0839, A0840, A0850 .6 .2 CD CB A1219, A1220, A1221 .8 .2 A1229, A1230, A1231 CE CB A2012, A2013, A2014, A2015 .7 .2 CF CC A2100, A2101, A2110, A2111 .4 .2 CB CA A2140, A2141, A2150, A2151 .5 .2 CB CA A2719, A2720, A2730 1.0 .2 CH CC A5520, A5530 .6 .4 CY CQ

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.