CAMPAIGN: HEATER INLET HOSE MISPOSITIONED CLAMP. Pontiac Fiero 1985

For 1990-2009 cars

# CAMPAIGN: HEATER INLET HOSE MISPOSITIONED CLAMP

GENERAL MOTORS HAS DETERMINED THAT CERTAIN 1984 PONTIAC FIERO MODELS WERE ASSEMBLED WITH A MISPOSITIONED UPPER RETAINING CLAMP ON THE HEATER INLET HOSE. THIS COULD ALLOW THE HOSE TO LOOSEN AND SEPARATE FROM THE HEATER INLET PIPE. A SEPARATED HOSE COULD CAUSE A LOSS OF ENGINE COOLANT WHICH COULD RESULT IN ENGINE FAILURE. VEHICLES INVOLVED INVOLVED ARE ONLY CERTAIN 1984 PONTIAC FIERO MODELS WITHIN THE FOLLOWING VEHICLE BREAKPOINTS: ASSEMBLY BEGINNING UP TO AND MODEL PLANT VIN INCLUDING 1984 FIERO PONTIAC (P) EP334595 EP334890 PART I - SERVICE PROCEDURE 1. RAISE REAR DECK. 2. REMOVE HEAT SHIELD (2 UPPER NUTS, 1 LOWER BOLT) THAT COVERS HEATER HOSES AND A/C LINES ALONG FRONT WALL OF ENGINE COMPARTMENT. 3. LOOSEN UPPER CLAMP ON HEATER INLET HOSE. 4. REPOSITION HOSE BEYOND SECOND RIB ON HEATER INLET PIPE (SEE FIGURE 1). 5. POSITION CLAMP BETWEEN THE TWO INLET PIPE RIBS AND RETIGHTEN TO 2 N.M OR 16 IN. LBS. 6. REINSTALL HEAT SHIELD. 7. SEE PART II FOR INSTALLATION OF CAMPAIGN IDENTIFICATION LABEL.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.