INOPERATIVE ODOMETER REGISTER ADDITIONAL MILEAGE. Pontiac Fiero 1986

For 1990-2009 cars

# INOPERATIVE ODOMETER REGISTER ADDITIONAL MILEAGE

#### CONDITION:

ON SOME 1986 FIERO MODELS, THE ODOMETER WILL NOT REGISTER ADDITIONAL MILEAGE OR THE 10 AMP GAGE FUSE WILL BLOW. CAUSE: THE ODOMETER STEPPER MOTOR RIBBON CABLE SHORTS AGAINST THE SPEEDOMETER CIRCUIT BOARD. ONLY FIERO VEHICLES EQUIPPED WITH V6 ENGINES ARE AFFECTED. CORRECTION: RETURN DEFECTIVE ODOMETERS/SPEEDOMETERS TO AN AUTHORIZED AC SPARK PLUG SERVICE CENTER FOR REPAIR. VEHICLES AFTER VIN GP207255 HAVE BEEN CORRECTED.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.