AUXILIARY COOLING FAN DUCTS INSUFFICIENT COOL AIR. Pontiac Fiero 1985

For 1990-2009 cars

# AUXILIARY COOLING FAN DUCTS INSUFFICIENT COOL AIR

#### VEHICLES AFFECTED: 1985 Fiero With V-6 Engine

#### CONDITION:

---------- Insufiicient cool air is emitted from the alternator and ignition coil auxiliary cooling fan ducts.

#### CAUSE:

------ The cooling fan motor connector is wired backward.

#### CORRECTION:

---------- (1) Locate the white two wire connector at the right hand side of the rear compartment. (The insulation must be pulled away from the trunk wall at the right side to access this connector.)

(2) A black wire with a red stripe should be located in cavity 'A' of the connector.

(A) If it is not, install it in cavity 'A', then install the remaining black wire in cavity 'B' of the connector.

(B) Test wire installation by performing push, pull test. After pushing and pulling on each individual wire, the wire should not separate from the connector.

(3) With ignition on and in A/C mode (engine not running) check blower performance for increased output.

(4) VIN's after FP 267813 built after August 1, 1985 should have corrected wiring.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.