INOP. 'DOOR AJAR' SWITCH REPLACE MALFUNCTIONING SWITCH. Pontiac Fiero 1986

For 1990-2009 cars

# INOP. 'DOOR AJAR' SWITCH REPLACE MALFUNCTIONING SWITCH

#### VEHICLES AFFECTED: 1986 Fiero

#### CONDITION:

--------- On some 1986 Fiero vehicles, the door ajar light may not function properly. Either the ajar light will not come on with the door open, or the ajar light will stay on with the door closed.

#### CAUSE:

----- The switch may not function properly due to the switch wiring and switch contacts being incompatible for durable operation.

#### CORRECTION:

---------- Replace malfunctioning ajar switches with the same part number switch. Fiero models built after September, 1985 commencing with V.I.N. GP212466 have revised switches.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.