FUEL PUMP SENDER INOPERATIVE BLOWN FUSE- FUEL PUMP. Pontiac Fiero 1984

For 1990-2009 cars

# FUEL PUMP SENDER INOPERATIVE BLOWN FUSE- FUEL PUMP

CONDITION: NO START OR RUN CONDITION DUE TO AN INOPERATIVE ELECTRIC FUEL PUMP SENDER UNIT AND/OR FUEL PUMP FUSE IS BLOWN. CAUSE: RADIO FILTER NETWORK ON THE FUEL LEVEL SENDER UNIT SHORT CIRCUITS. CORRECTION: REPLACE FUEL LEVEL SENDER UNIT (IDENTIFIED BY BLACK R.F.I. FILTER NETWORK ON TOP OF ELECTRIC FUEL PUMP) WITH THE SAME PART NUMBER FUEL LEVEL. SENDER UNIT (IDENTIFIED BY WHITE COLOR), P/N 25003251. NOTICE: ALL SENDERS WITH WHITE COLOR R.F.I. FILTER NETWORKS CAN BE USED. SENDERS WITH BLACK COLOR R.F.I. FILTER NETWORKS CAN BE USED AFTER JULIAN DATE CODE 0864 (MARCH 26, 1984). AS SHOWN IN THE ILLUSTRATION, THE FOUR DIGIT DATE CODE IS LOCATED ON A YELLOW TAG ON THE SENDER WIRE HARNESS AND ALSO ON THE ELECTRIC FUEL PUMP BODY.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.