ACCELERATOR CABLE CONTACTING DECK LID - REPOSITION CABLE. Pontiac Fiero 1984

For 1990-2009 cars

# ACCELERATOR CABLE CONTACTING DECK LID - REPOSITION CABLE

#### VEHICLES AFFECTED: 1984 & 1985 Fiero -----------------

#### CONDITION:

---------- Some 1984 and 1985 Fieros may show accelerator cable making contact with the rear deck lid which may result in chafing of the cable and/or deck lid.

#### CAUSE:

------ The condition may be caused by the routing of the cable and the rocking motion of the engine.

#### CORRECTION:

----------- Reposition cable as follows:

(1) Install stud 25517778 (torgue stud to 27 N.m), bracket 10028646, and nut 11507036 (torque nut to 20 N.m).

(2) Remove cable retainer clip 10029079 and place clip onto the bracket.

(3) Install cable to run across the rocker cover as illustrated. Move cable clip grommet along cable so that cable can be retained in clip.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.