For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 |

1. Connect a scan tool to the vehicle data link connector (DLC).
2. Enter the instrument cluster WOW mode.
3. Command the instrument cluster indicators on.

Does the check gauges indicator turn on?

--

Go to Powertrain On Board Diagnostic (OBD) System Check (V6 VIN K) or Powertrain On Board Diagnostic (OBD) System Check (V8 VIN G)

Go to Step 2

2 | Replace the instrument cluster. Refer to Instrument Cluster Replacement . Is the repair complete? | -- | System OK | --