For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 |

1. Turn the headlamps on.
2. Place the multi-function lever in the high beam position.
3. Observe the headlamps.

Do the high beam headlamps operate?

--

Go to Step 2

Go to Headlights: (DRL)

2 |

1. Remove the instrument cluster.
2. Connect a test lamp from the instrument cluster connector terminal A17 to ground.
3. Turn the headlamps on.
4. Place the multi-function lever in the high beam position.

Does the test lamp light?

--

Go to Step 3

Go to Step 4

3 |

1. Check for a poor connection at the instrument cluster connector terminal A17.
2. If the connection is OK, replace the instrument cluster. Refer to Instrument Cluster Replacement .

Is the repair complete?

--

System OK

--

4 | Repair the open in circuit 11. Is the repair complete? | -- | System OK | --