For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Remove the key from the ignition lock key cylinder.
2. Close both of the vehicle doors.
3. Observe the door locks while you press the driver door lock switch to the lock position.

Both of the doors lock when you press the driver door lock switch.

• | Power Door Locks - Lock Inoperative Unlock Operates

• | Power Door Locks Inoperative

• | Power Door Locks Switch Lock Function Inoperative - One

2 | Observe the door locks while you press the driver door lock switch to the unlock position. | Both of the doors unlock when you press the driver door unlock switch. |

• | Power Door Locks - Unlock Inoperative Lock Operates

• | Power Door Locks Inoperative

• | Power Door Locks Switch Unlock Function Inoperative - One

3 | Observe the door locks while you press the passenger door lock switch to the lock position. | Both of the doors lock when you press the passenger door lock switch. |

• | Power Door Locks - Lock Inoperative Unlock Operates

• | Power Door Locks Inoperative

• | Power Door Locks Switch Lock Function Inoperative - One

4 | Observe the door locks while you press the passenger door lock switch to the unlock position. | Both of the doors unlock when you press the passenger door unlock switch. |

• | Power Door Locks - Unlock Inoperative Lock Operates

• | Power Door Locks Inoperative

• | Power Door Locks Switch Unlock Function Inoperative - One

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.