For 1990-2009 cars

### Removal Procedure

Important: The automatic transmission control lever solenoid is a part of the brake transmission shift interlock (BTSI) system. The solenoid prevents the operator from shifting the automatic transmission control out of the PARK position unless the brake pedal is depressed.

1. Remove the front floor console trim plate. Refer to Console Trim Plate Replacement in Instrument Panel, Gauges, and Console.
2. Disconnect the electrical connector from the shift interlock solenoid.
3. Remove the shift interlock solenoid by unsnapping the retainers.

### Installation Procedure

1. Install the shift interlock solenoid. Snap the retainers into place.
2. Connect the electrical connector to the shift interlock solenoid.
3. Install the front floor console trim plate. Refer to Console Trim Plate Replacement in Instrument Panel, Gauges, and Console.